鴿隻感應傳輸

鴿會3碼,鴿舍5碼,環號6碼,電子鋁片號9碼,UID碼16碼,經EXXX.XXXXXX緯NXX.XXXXXX度,掌中寶感應時間MMDDhhmmss,傳送收到時間MMDDhhmmss,訊號強度(0-100),電量(0-100),是否充電(1插電0未插電), **460001357924680** (IMEI),伺服器接收時間MMDDhhmmss,狀態碼(101鴿隻上傳資訊999是單純測試)

參考格式

{"pigeon\_aluminum":"010100216","status\_code":"101","IMEI":"460001357924680","latitude":"N24.185225","longitude":"E120.699790","signal\_strength":"60","Electricity":"90","aluminum\_UID":"DDAC5004D00104E0","plugged\_in":"1","pigeon\_club":"001","UDP\_receive\_time":"0430094934","server\_receive\_time":"0430094947","induction\_time":"0430094904","pigeon\_loft":"01764","pigeon\_number":"031764"}

掌中寶狀態

鴿會3碼,鴿舍5碼, 掌中寶當下時間MMDDhhmmss, 經EXXX.XXXXXX度,緯NXX.XXXXXX度, ,訊號強度(0-100),電量(0-100),是否充電(1插電0未插電), **460001357924680** (IMEI),伺服器接收時間MMDDhhmmss,狀態碼(100是初次掌中寶傳輸300是後續狀態更新999是單純測試)

參考格式

{"status\_code":"000","longitude":"E120.699790","IMEI":"460001357924680","palm\_treasure\_time":"0430094904","Electricity":"90","latitude":"N24.185225","server\_receive\_time":"0430094947","plugged\_in":"1","pigeon\_club":"001","pigeon\_loft":"01764","signal\_strength":"60"}